# Board database 
Note: The're no differences between 48 and 64-pin MCUs layouts, they use the same pin names, thus the same firmware applies.<br><br> 
## Ksger v1
First generation KSGER, all boards have a 7-pin OLED connector, no other versions seem to exist.<br>
<br>
<img src="/Readme_files/boards/ksger_v1.jpg">
<br>

## Ksger v2
Second generation KSGER, all boards have a 4-pin OLED connector.<br>
This is the most common layout used by other parties like Quecoo, Quicko, JCD, Handskit...

#### Bad LDO design! Read [LDO issues](https://github.com/deividAlfa/stm32_soldering_iron_controller#ksger-self-resetting)
<img src="/Readme_files/boards/ksger_v2_1.jpg">

#### Bad LDO design! Read [LDO issues](https://github.com/deividAlfa/stm32_soldering_iron_controller#ksger-self-resetting)
<img src="/Readme_files/boards/ksger_v2_2.jpg">

<img src="/Readme_files/boards/ksger_v2_3.jpg">

<img src="/Readme_files/boards/ksger_v2_4.jpg">

<img src="/Readme_files/boards/ksger_v2_5.jpg">

<img src="/Readme_files/boards/ksger_v2_6.jpg">

<img src="/Readme_files/boards/ksger_v2_7.jpg">

<img src="/Readme_files/boards/ksger_v2_8.jpg">
<br>

## Ksger v3
Third generation KSGER, all boards have a 6-pin OLED connector, this layout is also used in other controllers.<br>

#### Bad LDO design! Read [LDO issues](https://github.com/deividAlfa/stm32_soldering_iron_controller#ksger-self-resetting)
<img src="/Readme_files/boards/ksger_v3_1.jpg">

#### Bad LDO design! Read [LDO issues](https://github.com/deividAlfa/stm32_soldering_iron_controller#ksger-self-resetting)
<img src="/Readme_files/boards/ksger_v3_2.jpg">

<img src="/Readme_files/boards/ksger_v3_3.jpg">

#### Bad LDO design! Read [LDO issues](https://github.com/deividAlfa/stm32_soldering_iron_controller#ksger-self-resetting)
<img src="/Readme_files/boards/ksger_v3_4.jpg">
<br>

## Quicko F072 / F103
The board is the same for both, only the cpu changes, has a 7-pin OLED connector.<br>
Check whether it has a STM32F072 or STM32F103 and choose the correct firmware accordingly.<br>
<br>
<img src="/Readme_files/boards/quicko.jpg">
<br>
